{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["非开挖修复材料"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"非开挖修复材料","index":0,"n_rows":36,"n_cols":7,"rows_kept":36,"merged":[[0,0,0,1],[1,0,1,6],[2,0,2,6],[4,3,8,3],[4,6,8,6],[9,6,11,6],[12,3,24,3],[12,6,24,6],[25,3,29,3],[25,6,29,6],[30,0,30,6],[31,0,31,5],[32,0,32,5],[33,0,33,5],[34,0,34,5],[35,0,35,5]],"flags":["formulas_cached_only"]}
["附件"]
["惠州市水电建筑工程有限公司2025年度非开挖修复材料采购项目（第二次）询价报价表"]
["类别：非开挖修复材料"]
["序号","材料名称","规格型号或指标","技术参数","单位","报价（元）","备注"]
[1,"紫外光固化玻璃纤维软管","DN300×3(mm)","1、内衬软管在储存、运输过程中应保持在厂家要求的温度下不会受到阳光照射。\n2、扎头应捆扎牢固。\n3、充气时每分钟加压10mPa,当气压达到100mPa时,每分钟加压50mPa,当气压到达200mPa时保压40min,同时做好紫外线固化准备。\n4、初始固化阶段紫外线灯行走速度宜控制在0.2~0.3m/min。软管固化过程中应观察控制台显示屏的紫外灯架行走里程并留意线缆标记。当紫外灯架距离终点0.5m时,紫外灯行走速度控制在0.2m/min。\n5、紫外线固化速度应按规定进行控制,修复过程中通过安装在紫外线前端的CCTV监控测点温度,随时调控温度。如有意外,及时停止进行处理。\n6、原位固化法内村管的短期力学性能的测试应按设计图纸力学性能要求表中的规定进行,并满足其规定的要求。内衬管的长期力学性能应根据业主的要求进行测试，不应小于初始性能的50%。","m",null,"紫外光原位固化法工艺"]
[2,"紫外光固化玻璃纤维软管","DN400×3(mm)",null,"m"]
[3,"紫外光固化玻璃纤维软管","DN500×4(mm)",null,"m"]
[4,"紫外光固化玻璃纤维软管","DN600×5(mm)",null,"m"]
[5,"紫外光固化玻璃纤维软管","DN800×6(mm)",null,"m"]
[6,"充气管堵","300～600(mm)","/","只",null,"管道临时封堵、注浆法工艺、点状原位固化法工艺"]
[7,"充气管堵","600～800(mm)","/","只"]
[8,"充气管堵","800～1200(mm)","/","只"]
[9,"不锈钢快速锁","DN300","不锈钢快速锁采用304或316号不锈钢套筒、三元乙丙橡胶套和锁紧机构等部件构成。各部分性能参数如下所示：\n1)DN600及以下的不锈钢套筒应由整片钢板加工成型，安装到位后应采用特殊锁紧装置固定；\n2)DN600以上的不锈钢套筒应由2片~3片加工好的不锈钢环片拼装而成，在安装到位后应采用专用锁紧螺栓固定；\n3)橡胶套应为闭合式，橡胶套外部两侧应设有整体式的密封凸台，性能指标应符合现行国家标准《橡胶密封件给、排水管及污水管道用接口密封圈材料规范》GB/T21873的有关规定。","环",null,"不锈钢快速锁法修复工艺"]
[10,"不锈钢快速锁","DN400",null,"环"]
[11,"不锈钢快速锁","DN500",null,"环"]
[12,"不锈钢快速锁","DN600",null,"环"]
[13,"不锈钢快速锁","DN800",null,"环"]
[14,"不锈钢快速锁","DN900",null,"环"]
[15,"不锈钢快速锁","DN1000",null,"环"]
[16,"不锈钢快速锁","DN1200",null,"环"]
[17,"不锈钢快速锁","DN1500",null,"环"]
[18,"密封橡胶套","F/300-L400",null,"个"]
[19,"密封橡胶套","F/400-L400",null,"个"]
[20,"密封橡胶套","F/500-L500",null,"个"]
[21,"密封橡胶套","F/600-L500",null,"个"]
[22,"密封橡胶套","F/800-L300","不锈钢快速锁采用304或316号不锈钢套筒、三元乙丙橡胶套和锁紧机构等部件构成。各部分性能参数如下所示：\n1)DN600及以下的不锈钢套筒应由整片钢板加工成型，安装到位后应采用特殊锁紧装置固定；\n2)DN600以上的不锈钢套筒应由2片~3片加工好的不锈钢环片拼装而成，在安装到位后应采用专用锁紧螺栓固定；\n3)橡胶套应为闭合式，橡胶套外部两侧应设有整体式的密封凸台，性能指标应符合现行国家标准《橡胶密封件给、排水管及污水管道用接口密封圈材料规范》GB/T21873的有关规定。","个",null,"不锈钢快速锁法修复工艺"]
[23,"密封橡胶套","F/900-L300",null,"个"]
[24,"密封橡胶套","F/1000-L300",null,"个"]
[25,"密封橡胶套","F/1200-L300",null,"个"]
[26,"密封橡胶套","F/1500-L300",null,"个"]
["注：1、单价包含材料费（包含配套材料、辅助材料等）、人工费、机械费、制作费、试验检测费、包装费、运杂费（包括装卸车费）、培训费、保险费、缺陷修复费、综合管理费、技术资料费、风险费、利润、各种税费、政策性文件规定费用等一切费用，即货物到达交货地点所发生的一切费用；数量以采购人实际采购数量为准，经验收合格后按送货量月结80%（进度款到账的情况下），当年结算至实际供货量的97%，实际供货款的3%作为质保金，质保金待完工一年后付清，具体以签订的合同条款为准。\n2、非开挖修复所使用的材料及工艺须满足《城镇排水管道非开挖修复工程施工及验收规程》中的相关规定。"]
["供应商名称："]
["供应商地址："]
["联系人："]
["联系电话："]
["日    期："]