{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["预制检查井","雨水口","井盖"],"not_rendered":{"external_links":1,"defined_names":9},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"预制检查井","index":0,"n_rows":325,"n_cols":8,"rows_kept":325,"merged":[[0,0,0,2],[1,0,1,7],[2,0,2,7],[3,1,3,2],[4,1,23,1],[24,1,32,1],[33,1,44,1],[45,1,52,1],[53,1,65,1],[66,1,70,1],[71,1,86,1],[87,1,88,1],[89,1,106,1],[108,1,124,1],[125,1,128,1],[129,1,149,1],[150,1,170,1],[171,1,191,1],[192,1,204,1],[205,1,212,1],[213,1,233,1],[234,1,254,1],[255,1,275,1],[276,1,288,1],[289,1,289,2],[290,1,290,2],[291,1,291,2],[292,1,292,2],[293,1,293,2],[294,1,294,2],[295,1,295,2],[296,1,296,2],[297,1,297,2],[298,1,298,2],[299,1,299,2],[300,1,300,2],[301,1,301,2],[302,1,302,2],[303,1,303,2],[304,1,304,2],[305,1,305,2],[306,1,306,2],[307,1,307,2],[308,1,308,2],[309,1,309,2],[310,1,310,2],[311,1,311,2],[312,1,312,2],[313,1,313,2],[314,1,314,2],[315,1,315,2],[316,1,316,2],[317,1,317,2],[318,1,318,2],[319,0,319,7],[320,0,320,6],[321,0,321,6],[322,0,322,6],[323,0,323,6],[324,0,324,6]],"flags":["formulas_cached_only"]}
["附件"]
["惠州市水电建筑工程有限公司2025-2026年度预制检查井、雨水口、井盖采购项目询价报价表"]
["类别：预制检查井"]
["序号","材料名称",null,"规格型号或指标","技术参数（详见国家建筑标准设计图集：20S515）","单位","报价（元）","备注"]
[1,"圆形检查井","雨水检查井","φ700","20S515,页21","m",null,"钢筋砼"]
[2,null,"污水检查井","φ700","20S515,页22","m",null,"钢筋砼"]
[3,null,"雨水检查井","φ800","20S515,页23","m",null,"钢筋砼"]
[4,null,"污水检查井","φ800","20S515,页24","m",null,"钢筋砼"]
[5,null,"雨水检查井","φ1000","20S515,页29","m",null,"钢筋砼 H=1.83m"]
[6,null,"雨水检查井","φ1000","20S515,页29","m",null,"钢筋砼 H=1.84m"]
[7,null,"雨水检查井","φ1000","20S515,页29","m",null,"钢筋砼 H=1.85m"]
[8,null,"雨水检查井","φ1000","20S515,页29","m",null,"钢筋砼 H=1.86m"]
[9,null,"雨水检查井","φ1250","20S515,页29","m",null,"钢筋砼 H=1.86m"]
[10,null,"雨水检查井","φ1250","20S515,页29","m",null,"钢筋砼 H=1.87m"]
[11,null,"雨水检查井","φ1250","20S515,页29","m",null,"钢筋砼 H=1.88m"]
[12,null,"雨水检查井","φ1500","20S515,页29","m",null,"钢筋砼 H=1.88m"]
[13,null,"雨水检查井","φ1500","20S515,页29","m",null,"钢筋砼 H=1.89m"]
[14,null,"雨水检查井","φ1500","20S515,页29","m",null,"钢筋砼 H=1.90m"]
[15,null,"雨水检查井","φ1800","20S515,页29","m",null,"钢筋砼 H=1.90m"]
[16,null,"雨水检查井","φ1800","20S515,页29","m",null,"钢筋砼 H=1.91m"]
[17,null,"污水检查井","φ1000","20S515,页30","m",null,"钢筋砼 H=2.03m"]
[18,null,"污水检查井","φ1000","20S515,页30","m",null,"钢筋砼 H=2.13m"]
[19,null,"污水检查井","φ1000","20S515,页30","m",null,"钢筋砼 H=2.24m"]
[20,null,"污水检查井","φ1000","20S515,页30","m",null,"钢筋砼 H=2.35m"]
[21,"圆形检查井","污水检查井","φ1000","20S515,页30","m",null,"钢筋砼 H=2.46m"]
[22,null,"污水检查井","φ1250","20S515,页30","m",null,"钢筋砼 H=2.46m"]
[23,null,"污水检查井","φ1250","20S515,页30","m",null,"钢筋砼 H=2.57m"]
[24,null,"污水检查井","φ1250","20S515,页30","m",null,"钢筋砼 H=2.68m"]
[25,null,"污水检查井","φ1500","20S515,页30","m",null,"钢筋砼 H=2.68m"]
[26,null,"污水检查井","φ1500","20S515,页30","m",null,"钢筋砼 H=2.79m"]
[27,null,"污水检查井","φ1500","20S515,页30","m",null,"钢筋砼 H=2.90m"]
[28,null,"污水检查井","φ1800","20S515,页30","m",null,"钢筋砼 H=2.90m"]
[29,null,"污水检查井","φ1800","20S515,页30","m",null,"钢筋砼 H=3.01m"]
[30,"矩形直线检查井","雨水检查井","1200×1100","20S515,页39","m",null,"钢筋砼 H=1.88m"]
[31,null,"雨水检查井","1400×1100","20S515,页39","m",null,"钢筋砼 H=1.90m"]
[32,null,"雨水检查井","1700×1100","20S515,页39","m",null,"钢筋砼 H=1.92m"]
[33,null,"雨水检查井","1900×1100","20S515,页39","m",null,"钢筋砼 H=1.94m"]
[34,null,"雨水检查井","2200×1100","20S515,页39","m",null,"钢筋砼 H=2.17m"]
[35,null,"雨水检查井","2400×1100","20S515,页39","m",null,"钢筋砼 H=2.41m"]
[36,null,"雨水检查井","2600×1100","20S515,页39","m",null,"钢筋砼 H=2.75m"]
[37,null,"雨水检查井","2900×1100","20S515,页39","m",null,"钢筋砼 H=2.99m"]
[38,null,"雨水检查井","3100×1100","20S515,页39","m",null,"钢筋砼 H=3.23m"]
[39,null,"雨水检查井","3400×1100","20S515,页39","m",null,"钢筋砼 H=3.47m"]
[40,null,"雨水检查井","3600×1100","20S515,页39","m",null,"钢筋砼 H=3.71m"]
[41,null,"雨水检查井","3900×1100","20S515,页39","m",null,"钢筋砼 H=3.95m"]
[42,"矩形直线检查井","污水检查井","1200×1100","20S515,页43","m",null,"钢筋砼 H=2.68m"]
[43,null,"污水检查井","1400×1100","20S515,页43","m",null,"钢筋砼 H=2.90m"]
[44,null,"污水检查井","1700×1100","20S515,页43","m",null,"钢筋砼 H=3.12m"]
[45,null,"污水检查井","1900×1100","20S515,页43","m",null,"钢筋砼 H=3.34m"]
[46,null,"污水检查井","2200×1100","20S515,页43","m",null,"钢筋砼 H=3.56m"]
[47,null,"污水检查井","2400×1100","20S515,页43","m",null,"钢筋砼 H=3.78m"]
[48,null,"污水检查井","2600×1100","20S515,页43","m",null,"钢筋砼 H=4.00m"]
[49,null,"污水检查井","2900×1100","20S515,页43","m",null,"钢筋砼 H=4.22m"]
[50,"矩形三通检查井","雨水检查井","1700×1700","20S515,页59","m",null,"钢筋砼 H=1.90m"]
[51,null,"雨水检查井","2100×2100","20S515,页59","m",null,"钢筋砼 H=1.92m"]
[52,null,"雨水检查井","2400×2400","20S515,页59","m",null,"钢筋砼 H=1.94m"]
[53,null,"雨水检查井","2700×2700","20S515,页59","m",null,"钢筋砼 H=2.17m"]
[54,null,"雨水检查井","3000×3000","20S515,页59","m",null,"钢筋砼 H=2.41m"]
[55,null,"雨水检查井","3300×3300","20S515,页59","m",null,"钢筋砼 H=2.75m"]
[56,null,"雨水检查井","3700×3700","20S515,页59","m",null,"钢筋砼 H=2.99m"]
[57,null,"雨水检查井","4000×4000","20S515,页59","m",null,"钢筋砼 H=3.23m"]
[58,null,"雨水检查井","4300×4300","20S515,页59","m",null,"钢筋砼 H=3.47m"]
[59,null,"雨水检查井","4600×4600","20S515,页59","m",null,"钢筋砼 H=3.71m"]
[60,null,"雨水检查井","5000×5000","20S515,页59","m",null,"钢筋砼 H=3.95m"]
[61,null,"污水检查井","1700×1700","20S515,页64","m",null,"钢筋砼 H=2.90m"]
[62,null,"污水检查井","2100×2100","20S515,页64","m",null,"钢筋砼 H=3.12m"]
[63,"矩形三通检查井","污水检查井","2400×2400","20S515,页64","m",null,"钢筋砼 H=3.34m"]
[64,null,"污水检查井","2700×2700","20S515,页64","m",null,"钢筋砼 H=3.56m"]
[65,null,"污水检查井","3000×3000","20S515,页64","m",null,"钢筋砼 H=3.78m"]
[66,null,"污水检查井","3300×3300","20S515,页64","m",null,"钢筋砼 H=4.00m"]
[67,null,"污水检查井","3700×3700","20S515,页64","m",null,"钢筋砼 H=4.22m"]
[68,"矩形四通检查井","雨水检查井","2000×1700","20S515,页80","m",null,"钢筋砼 H=1.90m"]
[69,null,"雨水检查井","2400×2100","20S515,页80","m",null,"钢筋砼 H=1.92m"]
[70,null,"雨水检查井","2800×2400","20S515,页80","m",null,"钢筋砼 H=1.94m"]
[71,null,"雨水检查井","3200×2700","20S515,页80","m",null,"钢筋砼 H=2.17m"]
[72,null,"雨水检查井","3600×3000","20S515,页80","m",null,"钢筋砼 H=2.41m"]
[73,null,"雨水检查井","4000×3300","20S515,页80","m",null,"钢筋砼 H=2.75m"]
[74,null,"雨水检查井","4400×3700","20S515,页80","m",null,"钢筋砼 H=2.99m"]
[75,null,"雨水检查井","4800×4000","20S515,页80","m",null,"钢筋砼 H=3.23m"]
[76,null,"雨水检查井","5200×4300","20S515,页80","m",null,"钢筋砼 H=3.47m"]
[77,null,"雨水检查井","5600×4600","20S515,页80","m",null,"钢筋砼 H=3.71m"]
[78,null,"雨水检查井","6000×5000","20S515,页80","m",null,"钢筋砼 H=3.95m"]
[79,null,"污水检查井","2000×1700","20S515,页85","m",null,"钢筋砼 H=2.90m"]
[80,null,"污水检查井","2400×2100","20S515,页85","m",null,"钢筋砼 H=3.12m"]
[81,null,"污水检查井","2800×2400","20S515,页85","m",null,"钢筋砼 H=3.34m"]
[82,null,"污水检查井","3200×2700","20S515,页85","m",null,"钢筋砼 H=3.56m"]
[83,null,"污水检查井","3600×3000","20S515,页85","m",null,"钢筋砼 H=3.78m"]
[84,"矩形四通检查井","污水检查井","4000×3300","20S515,页85","m",null,"钢筋砼 H=4.00m"]
[85,null,"污水检查井","4400×3700","20S515,页85","m",null,"钢筋砼 H=4.22m"]
[86,"矩形小三通检查井","雨水检查井","1700×1500","20S515,页122","m",null,"钢筋砼 H=1.90m"]
[87,null,"雨水检查井","2100×1800","20S515,页122","m",null,"钢筋砼 H=1.92m"]
[88,null,"雨水检查井","2400×2000","20S515,页122","m",null,"钢筋砼 H=1.94m"]
[89,null,"雨水检查井","2700×2300","20S515,页122","m",null,"钢筋砼 H=2.17m"]
[90,null,"雨水检查井","3000×2500","20S515,页122","m",null,"钢筋砼 H=2.41m"]
[91,null,"雨水检查井","3300×2800","20S515,页122","m",null,"钢筋砼 H=2.75m"]
[92,null,"雨水检查井","3700×3100","20S515,页122","m",null,"钢筋砼 H=2.99m"]
[93,null,"雨水检查井","4000×3400","20S515,页122","m",null,"钢筋砼 H=3.23m"]
[94,null,"雨水检查井","4300×3700","20S515,页122","m",null,"钢筋砼 H=3.47m"]
[95,null,"雨水检查井","4600×4000","20S515,页122","m",null,"钢筋砼 H=3.71m"]
[96,null,"雨水检查井","5000×4300","20S515,页122","m",null,"钢筋砼 H=3.95m"]
[97,null,"污水检查井","1700×1500","20S515,页127","m",null,"钢筋砼 H=2.90m"]
[98,null,"污水检查井","2100×1800","20S515,页127","m",null,"钢筋砼 H=3.12m"]
[99,null,"污水检查井","2400×2000","20S515,页127","m",null,"钢筋砼 H=3.34m"]
[100,null,"污水检查井","2700×2300","20S515,页127","m",null,"钢筋砼 H=3.56m"]
[101,null,"污水检查井","3000×2500","20S515,页127","m",null,"钢筋砼 H=3.78m"]
[102,null,"污水检查井","3300×2800","20S515,页127","m",null,"钢筋砼 H=4.00m"]
[103,null,"污水检查井","3700×3100","20S515,页127","m",null,"钢筋砼 H=4.22m"]
[104,"矩形小四通检查井","雨水检查井","2000×1500","20S515,页143","m",null,"钢筋砼 H=1.90m"]
[105,"矩形小四通检查井","雨水检查井","2400×1800","20S515,页143","m",null,"钢筋砼 H=1.92m"]
[106,null,"雨水检查井","2800×2000","20S515,页143","m",null,"钢筋砼 H=1.94m"]
[107,null,"雨水检查井","3200×2300","20S515,页143","m",null,"钢筋砼 H=2.17m"]
[108,null,"雨水检查井","3600×2500","20S515,页143","m",null,"钢筋砼 H=2.41m"]
[109,null,"雨水检查井","4000×2800","20S515,页143","m",null,"钢筋砼 H=2.75m"]
[110,null,"雨水检查井","4400×3100","20S515,页143","m",null,"钢筋砼 H=2.99m"]
[111,null,"雨水检查井","4800×3400","20S515,页143","m",null,"钢筋砼 H=3.23m"]
[112,null,"雨水检查井","5200×3700","20S515,页143","m",null,"钢筋砼 H=3.47m"]
[113,null,"雨水检查井","5600×4000","20S515,页143","m",null,"钢筋砼 H=3.71m"]
[114,null,"雨水检查井","6000×4300","20S515,页143","m",null,"钢筋砼 H=3.95m"]
[115,null,"污水检查井","2000×1500","20S515,页148","m",null,"钢筋砼 H=2.90m"]
[116,null,"污水检查井","2400×1800","20S515,页148","m",null,"钢筋砼 H=3.12m"]
[117,null,"污水检查井","2800×2000","20S515,页148","m",null,"钢筋砼 H=3.34m"]
[118,null,"污水检查井","3200×2300","20S515,页148","m",null,"钢筋砼 H=3.56m"]
[119,null,"污水检查井","3600×2500","20S515,页148","m",null,"钢筋砼 H=3.78m"]
[120,null,"污水检查井","4000×2800","20S515,页148","m",null,"钢筋砼 H=4.00m"]
[121,null,"污水检查井","4400×3100","20S515,页148","m",null,"钢筋砼 H=4.22m"]
[122,"扇形检查井","雨水检查井","A=1200，90°","20S515,页188","m",null,"钢筋砼 H=1.88m"]
[123,null,"雨水检查井","A=1400，90°","20S515,页188","m",null,"钢筋砼 H=1.90m"]
[124,null,"雨水检查井","A=1700，90°","20S515,页188","m",null,"钢筋砼 H=1.92m"]
[125,null,"雨水检查井","A=1900，90°","20S515,页188","m",null,"钢筋砼 H=1.94m"]
[126,"扇形检查井","雨水检查井","A=2200，90°","20S515,页188","m",null,"钢筋砼 H=2.17m"]
[127,null,"雨水检查井","A=2400，90°","20S515,页188","m",null,"钢筋砼 H=2.41m"]
[128,null,"雨水检查井","A=2600，90°","20S515,页188","m",null,"钢筋砼 H=2.75m"]
[129,null,"雨水检查井","A=2900，90°","20S515,页188","m",null,"钢筋砼 H=2.99m"]
[130,null,"雨水检查井","A=3100，90°","20S515,页188","m",null,"钢筋砼 H=3.23m"]
[131,null,"雨水检查井","A=3400，90°","20S515,页188","m",null,"钢筋砼 H=3.47m"]
[132,null,"雨水检查井","A=3600，90°","20S515,页188","m",null,"钢筋砼 H=3.71m"]
[133,null,"雨水检查井","A=3900，90°","20S515,页188","m",null,"钢筋砼 H=3.95m"]
[134,null,"雨水检查井","A=1200，120°","20S515,页188","m",null,"钢筋砼 H=1.88m"]
[135,null,"雨水检查井","A=1400，120°","20S515,页188","m",null,"钢筋砼 H=1.90m"]
[136,null,"雨水检查井","A=1700，120°","20S515,页188","m",null,"钢筋砼 H=1.92m"]
[137,null,"雨水检查井","A=1900，120°","20S515,页188","m",null,"钢筋砼 H=1.94m"]
[138,null,"雨水检查井","A=2200，120°","20S515,页188","m",null,"钢筋砼 H=2.17m"]
[139,null,"雨水检查井","A=2400，120°","20S515,页188","m",null,"钢筋砼 H=2.41m"]
[140,null,"雨水检查井","A=2600，120°","20S515,页188","m",null,"钢筋砼 H=2.75m"]
[141,null,"雨水检查井","A=2900，120°","20S515,页188","m",null,"钢筋砼 H=2.99m"]
[142,null,"雨水检查井","A=3100，120°","20S515,页188","m",null,"钢筋砼 H=3.23m"]
[143,null,"雨水检查井","A=3400，120°","20S515,页188","m",null,"钢筋砼 H=3.47m"]
[144,null,"雨水检查井","A=3600，120°","20S515,页188","m",null,"钢筋砼 H=3.71m"]
[145,null,"雨水检查井","A=3900，120°","20S515,页188","m",null,"钢筋砼 H=3.95m"]
[146,null,"雨水检查井","A=1200，135°","20S515,页188","m",null,"钢筋砼 H=1.88m"]
[147,"扇形检查井","雨水检查井","A=1400，135°","20S515,页188","m",null,"钢筋砼 H=1.90m"]
[148,null,"雨水检查井","A=1700，135°","20S515,页188","m",null,"钢筋砼 H=1.92m"]
[149,null,"雨水检查井","A=1900，135°","20S515,页188","m",null,"钢筋砼 H=1.94m"]
[150,null,"雨水检查井","A=2200，135°","20S515,页188","m",null,"钢筋砼 H=2.17m"]
[151,null,"雨水检查井","A=2400，135°","20S515,页188","m",null,"钢筋砼 H=2.41m"]
[152,null,"雨水检查井","A=2600，135°","20S515,页188","m",null,"钢筋砼 H=2.75m"]
[153,null,"雨水检查井","A=2900，135°","20S515,页188","m",null,"钢筋砼 H=2.99m"]
[154,null,"雨水检查井","A=3100，135°","20S515,页188","m",null,"钢筋砼 H=3.23m"]
[155,null,"雨水检查井","A=3400，135°","20S515,页188","m",null,"钢筋砼 H=3.47m"]
[156,null,"雨水检查井","A=3600，135°","20S515,页188","m",null,"钢筋砼 H=3.71m"]
[157,null,"雨水检查井","A=3900，135°","20S515,页188","m",null,"钢筋砼 H=3.95m"]
[158,null,"雨水检查井","A=1200，150°","20S515,页188","m",null,"钢筋砼 H=1.88m"]
[159,null,"雨水检查井","A=1400，150°","20S515,页188","m",null,"钢筋砼 H=1.90m"]
[160,null,"雨水检查井","A=1700，150°","20S515,页188","m",null,"钢筋砼 H=1.92m"]
[161,null,"雨水检查井","A=1900，150°","20S515,页188","m",null,"钢筋砼 H=1.94m"]
[162,null,"雨水检查井","A=2200，150°","20S515,页188","m",null,"钢筋砼 H=2.17m"]
[163,null,"雨水检查井","A=2400，150°","20S515,页188","m",null,"钢筋砼 H=2.41m"]
[164,null,"雨水检查井","A=2600，150°","20S515,页188","m",null,"钢筋砼 H=2.75m"]
[165,null,"雨水检查井","A=2900，150°","20S515,页188","m",null,"钢筋砼 H=2.99m"]
[166,null,"雨水检查井","A=3100，150°","20S515,页188","m",null,"钢筋砼 H=3.23m"]
[167,null,"雨水检查井","A=3400，150°","20S515,页188","m",null,"钢筋砼 H=3.47m"]
[168,"扇形检查井","雨水检查井","A=3600，150°","20S515,页188","m",null,"钢筋砼 H=3.71m"]
[169,null,"雨水检查井","A=3900，150°","20S515,页188","m",null,"钢筋砼 H=3.95m"]
[170,null,"污水检查井","A=1200，90°","20S515,页196","m",null,"钢筋砼 H=2.68m"]
[171,null,"污水检查井","A=1400，90°","20S515,页196","m",null,"钢筋砼 H=2.90m"]
[172,null,"污水检查井","A=1700，90°","20S515,页196","m",null,"钢筋砼 H=3.12m"]
[173,null,"污水检查井","A=1900，90°","20S515,页196","m",null,"钢筋砼 H=3.34m"]
[174,null,"污水检查井","A=2200，90°","20S515,页196","m",null,"钢筋砼 H=3.56m"]
[175,null,"污水检查井","A=2400，90°","20S515,页196","m",null,"钢筋砼 H=3.78m"]
[176,null,"污水检查井","A=2600，90°","20S515,页196","m",null,"钢筋砼 H=4.00m"]
[177,null,"污水检查井","A=2900，90°","20S515,页196","m",null,"钢筋砼 H=4.22m"]
[178,null,"污水检查井","A=1200，120°","20S515,页196","m",null,"钢筋砼 H=2.68m"]
[179,null,"污水检查井","A=1400，120°","20S515,页196","m",null,"钢筋砼 H=2.90m"]
[180,null,"污水检查井","A=1700，120°","20S515,页196","m",null,"钢筋砼 H=3.12m"]
[181,null,"污水检查井","A=1900，120°","20S515,页196","m",null,"钢筋砼 H=3.34m"]
[182,null,"污水检查井","A=2200，120°","20S515,页196","m",null,"钢筋砼 H=3.56m"]
[183,null,"污水检查井","A=2400，120°","20S515,页196","m",null,"钢筋砼 H=3.78m"]
[184,null,"污水检查井","A=2600，120°","20S515,页196","m",null,"钢筋砼 H=4.00m"]
[185,null,"污水检查井","A=2900，120°","20S515,页196","m",null,"钢筋砼 H=4.22m"]
[186,null,"污水检查井","A=1200，135°","20S515,页196","m",null,"钢筋砼 H=2.68m"]
[187,null,"污水检查井","A=1400，135°","20S515,页196","m",null,"钢筋砼 H=2.90m"]
[188,null,"污水检查井","A=1700，135°","20S515,页196","m",null,"钢筋砼 H=3.12m"]
[189,"扇形检查井","污水检查井","A=1900，135°","20S515,页196","m",null,"钢筋砼 H=3.34m"]
[190,null,"污水检查井","A=2200，135°","20S515,页196","m",null,"钢筋砼 H=3.56m"]
[191,null,"污水检查井","A=2400，135°","20S515,页196","m",null,"钢筋砼 H=3.78m"]
[192,null,"污水检查井","A=2600，135°","20S515,页196","m",null,"钢筋砼 H=4.00m"]
[193,null,"污水检查井","A=2900，135°","20S515,页196","m",null,"钢筋砼 H=4.22m"]
[194,null,"污水检查井","A=1200，150°","20S515,页196","m",null,"钢筋砼 H=2.68m"]
[195,null,"污水检查井","A=1400，150°","20S515,页196","m",null,"钢筋砼 H=2.90m"]
[196,null,"污水检查井","A=1700，150°","20S515,页196","m",null,"钢筋砼 H=3.12m"]
[197,null,"污水检查井","A=1900，150°","20S515,页196","m",null,"钢筋砼 H=3.34m"]
[198,null,"污水检查井","A=2200，150°","20S515,页196","m",null,"钢筋砼 H=3.56m"]
[199,null,"污水检查井","A=2400，150°","20S515,页196","m",null,"钢筋砼 H=3.78m"]
[200,null,"污水检查井","A=2600，150°","20S515,页196","m",null,"钢筋砼 H=4.00m"]
[201,null,"污水检查井","A=2900，150°","20S515,页196","m",null,"钢筋砼 H=4.22m"]
[202,"跌水井","竖管式跌水井（直线内跌）","φ1250","20S515,页250","m",null,"钢筋砼 H=2.10m"]
[203,null,"竖管式跌水井（直线内跌）","φ1250","20S515,页250","m",null,"钢筋砼 H=2.75m"]
[204,null,"竖管式跌水井（直线内跌）","φ1250","20S515,页250","m",null,"钢筋砼 H=3.75m"]
[205,null,"竖管式跌水井（直线内跌）","φ1250","20S515,页250","m",null,"钢筋砼 H=4.75m"]
[206,null,"竖管式跌水井（直线内跌）","φ1250","20S515,页250","m",null,"钢筋砼 H=5.75m"]
[207,null,"竖管式跌水井（直线内跌）","φ1250","20S515,页250","m",null,"钢筋砼 H=6.75m"]
[208,null,"竖管式跌水井（支线内跌）","φ1250","20S515,页252","m",null,"钢筋砼 H=2.10m"]
[209,null,"竖管式跌水井（支线内跌）","φ1250","20S515,页252","m",null,"钢筋砼 H=2.75m"]
[210,"跌水井","竖管式跌水井（支线内跌）","φ1250","20S515,页252","m",null,"钢筋砼 H=3.75m"]
[211,null,"竖管式跌水井（支线内跌）","φ1250","20S515,页252","m",null,"钢筋砼 H=4.75m"]
[212,null,"竖管式跌水井（支线内跌）","φ1250","20S515,页252","m",null,"钢筋砼 H=5.75m"]
[213,null,"竖管式跌水井（支线内跌）","φ1250","20S515,页252","m",null,"钢筋砼 H=6.75m"]
[214,null,"矩形竖槽式跌水井（直线外跌）","2100×1000","20S515,页259","m",null,"钢筋砼 H=2.25m"]
[215,null,"矩形竖槽式跌水井（直线外跌）","2100×1000","20S515,页259","m",null,"钢筋砼 H=2.35m"]
[216,null,"矩形竖槽式跌水井（直线外跌）","2100×1000","20S515,页259","m",null,"钢筋砼 H=2.45m"]
[217,null,"矩形竖槽式跌水井（直线外跌）","2100×1000","20S515,页259","m",null,"钢筋砼 H=2.55m"]
[218,null,"矩形竖槽式跌水井（直线外跌）","2100×1000","20S515,页259","m",null,"钢筋砼 H=2.65m"]
[219,null,"矩形竖槽式跌水井（直线外跌）","2100×1000","20S515,页259","m",null,"钢筋砼 H=2.72m"]
[220,null,"矩形竖槽式跌水井（直线外跌）","2100×1000","20S515,页259","m",null,"钢筋砼 H=2.83m"]
[221,null,"矩形竖槽式跌水井（直线外跌）","2100×1000","20S515,页259","m",null,"钢筋砼 H=2.94m"]
[222,null,"矩形竖槽式跌水井（直线外跌）","2100×1000","20S515,页259","m",null,"钢筋砼 H=3.05m"]
[223,null,"矩形竖槽式跌水井（直线外跌）","2100×1000","20S515,页259","m",null,"钢筋砼 H=3.16m"]
[224,null,"矩形竖槽式跌水井（直线外跌）","2100×1000","20S515,页259","m",null,"钢筋砼 H=3.72m"]
[225,null,"矩形竖槽式跌水井（直线外跌）","2100×1000","20S515,页259","m",null,"钢筋砼 H=3.83m"]
[226,null,"矩形竖槽式跌水井（直线外跌）","2100×1000","20S515,页259","m",null,"钢筋砼 H=3.94m"]
[227,null,"矩形竖槽式跌水井（直线外跌）","2100×1000","20S515,页259","m",null,"钢筋砼 H=4.05m"]
[228,null,"矩形竖槽式跌水井（直线外跌）","2100×1000","20S515,页259","m",null,"钢筋砼 H=4.16m"]
[229,null,"矩形竖槽式跌水井（直线外跌）","2100×1000","20S515,页259","m",null,"钢筋砼 H=4.72m"]
[230,null,"矩形竖槽式跌水井（直线外跌）","2100×1000","20S515,页259","m",null,"钢筋砼 H=4.83m"]
[231,"跌水井","矩形竖槽式跌水井（直线外跌）","2100×1000","20S515,页259","m",null,"钢筋砼 H=4.94m"]
[232,null,"矩形竖槽式跌水井（直线外跌）","2100×1000","20S515,页259","m",null,"钢筋砼 H=5.05m"]
[233,null,"矩形竖槽式跌水井（直线外跌）","2100×1000","20S515,页259","m",null,"钢筋砼 H=5.16m"]
[234,null,"矩形竖槽式跌水井（单支线外跌）","2100×1000","20S515,页261","m",null,"钢筋砼 H=2.25m"]
[235,null,"矩形竖槽式跌水井（单支线外跌）","2100×1000","20S515,页261","m",null,"钢筋砼 H=2.35m"]
[236,null,"矩形竖槽式跌水井（单支线外跌）","2100×1000","20S515,页261","m",null,"钢筋砼 H=2.45m"]
[237,null,"矩形竖槽式跌水井（单支线外跌）","2100×1000","20S515,页261","m",null,"钢筋砼 H=2.55m"]
[238,null,"矩形竖槽式跌水井（单支线外跌）","2100×1000","20S515,页261","m",null,"钢筋砼 H=2.65m"]
[239,null,"矩形竖槽式跌水井（单支线外跌）","2100×1000","20S515,页261","m",null,"钢筋砼 H=2.72m"]
[240,null,"矩形竖槽式跌水井（单支线外跌）","2100×1000","20S515,页261","m",null,"钢筋砼 H=2.83m"]
[241,null,"矩形竖槽式跌水井（单支线外跌）","2100×1000","20S515,页261","m",null,"钢筋砼 H=2.94m"]
[242,null,"矩形竖槽式跌水井（单支线外跌）","2100×1000","20S515,页261","m",null,"钢筋砼 H=3.05m"]
[243,null,"矩形竖槽式跌水井（单支线外跌）","2100×1000","20S515,页261","m",null,"钢筋砼 H=3.16m"]
[244,null,"矩形竖槽式跌水井（单支线外跌）","2100×1000","20S515,页261","m",null,"钢筋砼 H=3.72m"]
[245,null,"矩形竖槽式跌水井（单支线外跌）","2100×1000","20S515,页261","m",null,"钢筋砼 H=3.83m"]
[246,null,"矩形竖槽式跌水井（单支线外跌）","2100×1000","20S515,页261","m",null,"钢筋砼 H=3.94m"]
[247,null,"矩形竖槽式跌水井（单支线外跌）","2100×1000","20S515,页261","m",null,"钢筋砼 H=4.05m"]
[248,null,"矩形竖槽式跌水井（单支线外跌）","2100×1000","20S515,页261","m",null,"钢筋砼 H=4.16m"]
[249,null,"矩形竖槽式跌水井（单支线外跌）","2100×1000","20S515,页261","m",null,"钢筋砼 H=4.72m"]
[250,null,"矩形竖槽式跌水井（单支线外跌）","2100×1000","20S515,页261","m",null,"钢筋砼 H=4.83m"]
[251,null,"矩形竖槽式跌水井（单支线外跌）","2100×1000","20S515,页261","m",null,"钢筋砼 H=4.94m"]
[252,"跌水井","矩形竖槽式跌水井（单支线外跌）","2100×1000","20S515,页261","m",null,"钢筋砼 H=5.05m"]
[253,null,"矩形竖槽式跌水井（单支线外跌）","2100×1000","20S515,页261","m",null,"钢筋砼 H=5.16m"]
[254,null,"阶梯式跌水井","2500×1200","20S515,页295","m",null,"钢筋砼 H=3.05m"]
[255,null,"阶梯式跌水井","2500×1400","20S515,页295","m",null,"钢筋砼 H=3.25m"]
[256,null,"阶梯式跌水井","2500×1700","20S515,页295","m",null,"钢筋砼 H=3.50m"]
[257,null,"阶梯式跌水井","2500×1900","20S515,页295","m",null,"钢筋砼 H=3.75m"]
[258,null,"阶梯式跌水井","2500×2200","20S515,页295","m",null,"钢筋砼 H=4.00m"]
[259,null,"阶梯式跌水井","2500×2400","20S515,页295","m",null,"钢筋砼 H=4.25m"]
[260,null,"阶梯式跌水井","2500×2600","20S515,页295","m",null,"钢筋砼 H=4.45m"]
[261,null,"阶梯式跌水井","2500×2900","20S515,页295","m",null,"钢筋砼 H=4.70m"]
[262,null,"阶梯式跌水井","3500×1200","20S515,页295","m",null,"钢筋砼 H=3.05m"]
[263,null,"阶梯式跌水井","3500×1400","20S515,页295","m",null,"钢筋砼 H=3.25m"]
[264,null,"阶梯式跌水井","3500×1700","20S515,页295","m",null,"钢筋砼 H=3.50m"]
[265,null,"阶梯式跌水井","3500×1900","20S515,页295","m",null,"钢筋砼 H=3.75m"]
[266,null,"阶梯式跌水井","3500×2200","20S515,页295","m",null,"钢筋砼 H=4.00m"]
[267,null,"阶梯式跌水井","3500×2400","20S515,页295","m",null,"钢筋砼 H=4.25m"]
[268,null,"阶梯式跌水井","3500×2600","20S515,页295","m",null,"钢筋砼 H=4.45m"]
[269,null,"阶梯式跌水井","3500×2900","20S515,页295","m",null,"钢筋砼 H=4.70m"]
[270,null,"阶梯式跌水井","4000×1200","20S515,页295","m",null,"钢筋砼 H=3.25m"]
[271,null,"阶梯式跌水井","4000×1400","20S515,页295","m",null,"钢筋砼 H=3.45m"]
[272,null,"阶梯式跌水井","4000×1700","20S515,页295","m",null,"钢筋砼 H=3.70m"]
[273,"跌水井","阶梯式跌水井","4000×1900","20S515,页295","m",null,"钢筋砼 H=3.95m"]
[274,null,"阶梯式跌水井","4000×2200","20S515,页295","m",null,"钢筋砼 H=4.20m"]
[275,null,"阶梯式跌水井","4000×2400","20S515,页295","m",null,"钢筋砼 H=4.45m"]
[276,null,"阶梯式跌水井","4000×2600","20S515,页295","m",null,"钢筋砼 H=4.75m"]
[277,null,"阶梯式跌水井","4000×2900","20S515,页295","m",null,"钢筋砼 H=5.00m"]
[278,null,"阶梯式跌水井","5000×1200","20S515,页295","m",null,"钢筋砼 H=3.75m"]
[279,null,"阶梯式跌水井","5000×1400","20S515,页295","m",null,"钢筋砼 H=3.95m"]
[280,null,"阶梯式跌水井","5000×1700","20S515,页295","m",null,"钢筋砼 H=4.20m"]
[281,null,"阶梯式跌水井","5000×1900","20S515,页295","m",null,"钢筋砼 H=4.45m"]
[282,null,"阶梯式跌水井","5000×2200","20S515,页295","m",null,"钢筋砼 H=4.70m"]
[283,null,"阶梯式跌水井","5000×2400","20S515,页295","m",null,"钢筋砼 H=4.95m"]
[284,null,"阶梯式跌水井","5000×2600","20S515,页295","m",null,"钢筋砼 H=5.25m"]
[285,null,"阶梯式跌水井","5000×2900","20S515,页295","m",null,"钢筋砼 H=5.50m"]
[286,"圆形沉泥井",null,"φ1000","20S515,页313","m",null,"钢筋砼 H=2.60m"]
[287,"圆形沉泥井",null,"φ1000","20S515,页313","m",null,"钢筋砼 H=2.70m"]
[288,"圆形沉泥井",null,"φ1000","20S515,页313","m",null,"钢筋砼 H=2.80m"]
[289,"圆形沉泥井",null,"φ1000","20S515,页313","m",null,"钢筋砼 H=2.90m"]
[290,"圆形沉泥井",null,"φ1250","20S515,页313","m",null,"钢筋砼 H=3.00m"]
[291,"圆形沉泥井",null,"φ1250","20S515,页313","m",null,"钢筋砼 H=3.10m"]
[292,"圆形沉泥井",null,"φ1500","20S515,页313","m",null,"钢筋砼 H=3.20m"]
[293,"圆形沉泥井",null,"φ1500","20S515,页313","m",null,"钢筋砼 H=3.30m"]
[294,"圆形沉泥井",null,"φ1500","20S515,页313","m",null,"钢筋砼 H=3.40m"]
[295,"污水闸槽井",null,"1200×1300","20S515,页317","m",null,"钢筋砼 H=2.20m"]
[296,"污水闸槽井",null,"1400×1300","20S515,页317","m",null,"钢筋砼 H=2.40m"]
[297,"污水闸槽井",null,"1600×1300","20S515,页317","m",null,"钢筋砼 H=2.60m"]
[298,"污水闸槽井",null,"1800×1300","20S515,页317","m",null,"钢筋砼 H=2.80m"]
[299,"污水闸槽井",null,"2000×1300","20S515,页317","m",null,"钢筋砼 H=3.00m"]
[300,"小方形户线检查井",null,"500×500","20S515,页324","座",null,"钢筋砼 H1=1.00m"]
[301,"小方形户线检查井",null,"500×500","20S515,页324","座",null,"钢筋砼 H1=1.50m"]
[302,"小方形户线检查井",null,"600×600","20S515,页326","座",null,"钢筋砼 H1=1.00m"]
[303,"小方形户线检查井",null,"600×600","20S515,页326","座",null,"钢筋砼 H1=1.50m"]
[304,"小方形户线检查井",null,"700×700","20S515,页328","座",null,"钢筋砼 H1=1.00m"]
[305,"小方形户线检查井",null,"700×700","20S515,页328","座",null,"钢筋砼 H1=1.50m"]
[306,"预制混凝土井筒",null,"φ700","20S515,页331","座",null,"钢筋砼 L=0.27m"]
[307,"预制混凝土井筒",null,"φ700","20S515,页331","座",null,"钢筋砼 L=0.36m"]
[308,"预制混凝土井筒",null,"φ700","20S515,页331","座",null,"钢筋砼 L=0.72m"]
[309,"预制混凝土井筒",null,"φ700","20S515,页331","座",null,"钢筋砼 L=1.44m"]
[310,"预制混凝土井筒",null,"φ700","20S515,页331","座",null,"钢筋砼 L=1.80m"]
[311,"预制混凝土井筒",null,"φ800","20S515,页331","座",null,"钢筋砼 L=0.27m"]
[312,"预制混凝土井筒",null,"φ800","20S515,页331","座",null,"钢筋砼 L=0.36m"]
[313,"预制混凝土井筒",null,"φ800","20S515,页331","座",null,"钢筋砼 L=0.72m"]
[314,"预制混凝土井筒",null,"φ800","20S515,页331","座",null,"钢筋砼 L=1.44m"]
[315,"预制混凝土井筒",null,"φ800","20S515,页331","座",null,"钢筋砼 L=1.80m"]
["注：1、单价包含材料费（包含配套材料、辅助材料等）、人工费、机械费、制作费、试验检测费、包装费、运杂费（包括装卸车费）、培训费、保险费、缺陷修复费、综合管理费、技术资料费、风险费、利润、各种税费、政策性文件规定费用等一切费用，即货物到达交货地点所发生的一切费用；数量以采购人实际采购数量为准，送货量月结80%，当年结算至97%，质量保证金3%完工一年后付清，具体以签订的合同条款为准。\n2、以上所有井室均包含底板、盖板，供应商报价时需一并考虑。"]
["供应商名称："]
["供应商地址："]
["联系人："]
["联系电话："]
["日    期："]

{"sheet":"雨水口","index":1,"n_rows":22,"n_cols":8,"rows_kept":22,"merged":[[0,0,0,2],[1,0,1,7],[2,0,2,7],[3,1,3,2],[4,1,4,2],[5,1,5,2],[6,1,6,2],[7,1,7,2],[8,1,8,2],[9,1,9,2],[10,1,10,2],[11,1,11,2],[12,1,12,2],[13,1,13,2],[14,1,14,2],[15,1,15,2],[16,0,16,7],[17,0,17,6],[18,0,18,6],[19,0,19,6],[20,0,20,6],[21,0,21,6]],"flags":["formulas_cached_only"]}
["附件"]
["惠州市水电建筑工程有限公司2025-2026年度预制检查井、雨水口、井盖采购项目询价报价表"]
["类别：雨水口"]
["序号","材料名称",null,"规格型号或指标","技术参数（详见国家建筑标准设计图集：16S518）","单位","报价（元）","备注"]
[1,"预制混凝土装配式平篦式单箅雨水口",null,"700*400","16S518，页39","座",null,"钢筋砼 H=0.72m"]
[2,"预制混凝土装配式平篦式单箅雨水口",null,"700*400","16S518，页39","座",null,"钢筋砼 H=0.94m"]
[3,"预制混凝土装配式平篦式双箅雨水口",null,"700*400","16S518，页40","座",null,"钢筋砼 H=0.72m"]
[4,"预制混凝土装配式平篦式双箅雨水口",null,"700*400","16S518，页40","座",null,"钢筋砼 H=0.94m"]
[5,"预制混凝土装配式平篦式三箅雨水口",null,"700*400","16S518，页41","座",null,"钢筋砼 H=0.72m"]
[6,"预制混凝土装配式平篦式三箅雨水口",null,"700*400","16S518，页41","座",null,"钢筋砼 H=0.94m"]
[7,"预制混凝土装配式偏沟式单箅雨水口",null,"700*400","16S518，页42","座",null,"钢筋砼 H=0.72m"]
[8,"预制混凝土装配式偏沟式单箅雨水口",null,"700*400","16S518，页42","座",null,"钢筋砼 H=0.94m"]
[9,"预制混凝土装配式偏沟式双箅雨水口",null,"700*400","16S518，页43","座",null,"钢筋砼 H=0.72m"]
[10,"预制混凝土装配式偏沟式双箅雨水口",null,"700*400","16S518，页43","座",null,"钢筋砼 H=0.94m"]
[11,"预制混凝土装配式偏沟式三箅雨水口",null,"700*400","16S518，页44","座",null,"钢筋砼 H=0.72m"]
[12,"预制混凝土装配式偏沟式三箅雨水口",null,"700*400","16S518，页44","座",null,"钢筋砼 H=0.94m"]
["注：1、单价包含材料费（包含配套材料、辅助材料等）、人工费、机械费、制作费、试验检测费、包装费、运杂费（包括装卸车费）、培训费、保险费、缺陷修复费、综合管理费、技术资料费、风险费、利润、各种税费、政策性文件规定费用等一切费用，即货物到达交货地点所发生的一切费用；数量以采购人实际采购数量为准，送货量月结80%，当年结算至97%，质量保证金3%完工一年后付清，具体以签订的合同条款为准。\n2、以上所有雨水口均包含底板，供应商报价时需一并考虑。"]
["供应商名称："]
["供应商地址："]
["联系人："]
["联系电话："]
["日    期："]

{"sheet":"井盖","index":2,"n_rows":20,"n_cols":8,"rows_kept":20,"merged":[[0,0,0,2],[1,0,1,7],[2,0,2,7],[3,1,3,2],[4,1,4,2],[4,4,11,4],[4,7,11,7],[5,1,5,2],[6,1,6,2],[7,1,7,2],[8,1,8,2],[9,1,9,2],[10,1,10,2],[11,1,11,2],[12,1,12,2],[12,7,13,7],[13,1,13,2],[14,0,14,7],[15,0,15,6],[16,0,16,6],[17,0,17,6],[18,0,18,6],[19,0,19,6]],"flags":["formulas_cached_only"]}
["附件"]
["惠州市水电建筑工程有限公司2025-2026年度预制检查井、雨水口、井盖采购项目询价报价表"]
["类别：井盖"]
["序号","材料名称",null,"规格型号或指标","技术参数（详见国家建筑标准设计图集：20S515、16S518）","单位","报价（元）","备注"]
[1,"球墨铸铁井盖连座（防沉降、含尼龙防坠网）",null,"重型φ800\nD400","检查井井盖所用的球墨铸铁应符合《球墨铸铁件》（GB/T1348-2019）的规定。","套",null,"井盖标识按使用方要求进行生产，井盖标有“生产日期、给水、雨水、污水、logo、执行标准、承压等级、权属单位信息等。"]
[2,"球墨铸铁井盖连座（防沉降、含尼龙防坠网）",null,"轻型φ800\nC250",null,"套"]
[3,"球墨铸铁井盖连座（防沉降、含尼龙防坠网）",null,"重型φ700\nD400",null,"套"]
[4,"球墨铸铁井盖连座（防沉降、含尼龙防坠网）",null,"轻型φ700\nC250",null,"套"]
[5,"球墨铸铁井盖连座（防沉降、含尼龙防坠网）",null,"重型φ600\nD400",null,"套"]
[6,"球墨铸铁井盖连座（防沉降、含尼龙防坠网）",null,"轻型φ600\nC250",null,"套"]
[7,"球墨铸铁井盖连座（防沉降、含尼龙防坠网）",null,"重型φ500\nD400",null,"套"]
[8,"球墨铸铁井盖连座（防沉降、含尼龙防坠网）",null,"轻型φ500\nC250",null,"套"]
[9,"铸铁平箅(防沉降、含支座、含配套截污挂篮）",null,"750×450","D400重型球墨铸铁箅子","套",null,"标识按使用方要求进行生产。"]
[10,"铸铁平箅(防沉降、含支座、含配套截污挂篮）",null,"750×450","C250轻型球墨铸铁箅子","套"]
["注：单价包含材料费（包含配套材料、辅助材料等）、人工费、机械费、制作费、试验检测费、包装费、运杂费（包括装卸车费）、培训费、保险费、缺陷修复费、综合管理费、技术资料费、风险费、利润、各种税费、政策性文件规定费用等一切费用，即货物到达交货地点所发生的一切费用；数量以采购人实际采购数量为准，送货量月结80%，当年结算至97%，质量保证金3%完工一年后付清，具体以签订的合同条款为准。"]
["供应商名称："]
["供应商地址："]
["联系人："]
["联系电话："]
["日    期："]